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…brings you your very own Raynor Lounge!

Soon the real thing will be gone for ever… but you can create a lasting memento of the old-style Raynor’ with this simple cut out and assemble kit. All you need is a pair of sharp scissors, some decent glue (UHU, not Pritt Stick), and a patient disposition!

Assembly instructions

A) constructing the basic room

1) Cut around the outside of the main Raynor Lounge structure.

2) Cut along the black line marking the bottom of the side wall, from the back wall to the bottom of the stage step (indicated by yellow line and text above).
3) Do the same on the opposite side wall.

4) Score and fold back the yellow tabs at the end of each side wall.

5) Score and fold along the lines where wall meets floor.

6) Carefully score and fold along the top and bottom of the stage step to create the step up.

7) Create the room structure by gluing the end of wall tabs to behind the adjacent wall – this completes the structure of the room.

B) adding the accessories

1) Cut out the DJ booth, pillar and metal bar that runs along the edge of the stage.
2) Use a pencil to curve the DJ booth card, and glue into marked position.

3) Score and fold corners of pillar, glue side tab to form it, and stick bottom tab to yellow shaded area on dancefloor.
4) Stick bar to front of stage step / back of pillar.
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